

Optimized paths

t: next time interval

w: next IoT input workload

p: next routs optimized by EPOS

Execute services

Move vehicles

Measure & evaluate

Connecting vehicles to the closest access points (AP)

Distribute w across vehicles

Place IoT services on the selected hosts

Sending requests from vehicles to the edge nodes



Generate plans regarding local-cost and future locations