j1

j3

j2

d2

d1

m

m

Access point/fog node

Mobile end-device

t0+∆t

t0